IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2025-02-25T19:42:20"
Preprocessor: "NORM3D - SCAN2BIM"
Originating system: "NORM3D - SCAN2BIM"
Application: "NORM3D - SCAN2BIM" version "2025" identifier "NORM3D - SCAN2BIM" by Organization "NORM3D - SCAN2BIM"

People and organizations
  Person "contact@norm3d.com" of Organization (no name given)
  Owner history of Person "contact@norm3d.com" of Organization (no name given) | application "NORM3D - SCAN2BIM" version "2025" identifier "NORM3D - SCAN2BIM" by Organization "NORM3D - SCAN2BIM" | change NOCHANGE | created 1740508940 (2025-02-25T18:42:20Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level 2" | elevation -0.350503951311111
        contains 43 elements
          20 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:1", "Wall:2", "Wall:3" (+17 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232)
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 880 x 1210mm" | object type "Window : 880 x 1210mm" | names: "Window : 880 x 1210mm : 0", "Window : 880 x 1210mm : 1", "Window : 880 x 1210mm : 10" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 920 x 1225mm" | object type "Window : 920 x 1225mm" | names: "Window : 920 x 1225mm : 2" | material: "Window Default"
          2 x IFCDOOR | type IFCDOORSTYLE "Door : 1010 x 2100mm" | object type "Door : 1010 x 2100mm" | names: "Door : 1010 x 2100mm : 0", "Door : 1010 x 2100mm : 2" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 920 x 1220mm" | object type "Window : 920 x 1220mm" | names: "Window : 920 x 1220mm : 3" | material: "Window Default"
          2 x IFCDOOR | type IFCDOORSTYLE "Door : 1010 x 2105mm" | object type "Door : 1010 x 2105mm" | names: "Door : 1010 x 2105mm : 1", "Door : 1010 x 2105mm : 4" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 945 x 1225mm" | object type "Window : 945 x 1225mm" | names: "Window : 945 x 1225mm : 4" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 900 x 1215mm" | object type "Window : 900 x 1215mm" | names: "Window : 900 x 1215mm : 5" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 905 x 1215mm" | object type "Window : 905 x 1215mm" | names: "Window : 905 x 1215mm : 6" | material: "Window Default"
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 925 x 1225mm" | object type "Window : 925 x 1225mm" | names: "Window : 925 x 1225mm : 7", "Window : 925 x 1225mm : 8" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 720 x 2125mm" | object type "Door : 720 x 2125mm" | names: "Door : 720 x 2125mm : 3" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 915 x 1215mm" | object type "Window : 915 x 1215mm" | names: "Window : 915 x 1215mm : 9" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 915 x 1220mm" | object type "Window : 915 x 1220mm" | names: "Window : 915 x 1220mm : 11" | material: "Window Default"
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
        IFCSPACE "Room 001"
        IFCSPACE "Room 002"
        IFCSPACE "Room 003"
        IFCSPACE "Room 004"
        IFCSPACE "Room 005"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level 1" | elevation -4.30057716369629
        contains 46 elements
          24 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "wall_thickness_0.2000" | object type "Wall" | names: "Wall:21", "Wall:22", "Wall:23" (+21 more) | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 925 x 1235mm" | object type "Window : 925 x 1235mm" | names: "Window : 925 x 1235mm : 12", "Window : 925 x 1235mm : 15", "Window : 925 x 1235mm : 20" (+1 more) | material: "Window Default"
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 910 x 1225mm" | object type "Window : 910 x 1225mm" | names: "Window : 910 x 1225mm : 13", "Window : 910 x 1225mm : 23", "Window : 910 x 1225mm : 24" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 1010 x 2100mm" | object type "Door : 1010 x 2100mm" | names: "Door : 1010 x 2100mm : 5" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 880 x 1215mm" | object type "Window : 880 x 1215mm" | names: "Window : 880 x 1215mm : 14" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 880 x 1210mm" | object type "Window : 880 x 1210mm" | names: "Window : 880 x 1210mm : 16" | material: "Window Default"
          2 x IFCDOOR | type IFCDOORSTYLE "Door : 1005 x 2100mm" | object type "Door : 1005 x 2100mm" | names: "Door : 1005 x 2100mm : 6", "Door : 1005 x 2100mm : 8" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 925 x 1230mm" | object type "Window : 925 x 1230mm" | names: "Window : 925 x 1230mm : 17" | material: "Window Default"
          1 x IFCDOOR | type IFCDOORSTYLE "Door : 1010 x 2105mm" | object type "Door : 1010 x 2105mm" | names: "Door : 1010 x 2105mm : 7" | material: "Door Panel"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 890 x 1215mm" | object type "Window : 890 x 1215mm" | names: "Window : 890 x 1215mm : 18" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 920 x 1225mm" | object type "Window : 920 x 1225mm" | names: "Window : 920 x 1225mm : 19" | material: "Window Default"
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window : 895 x 1215mm" | object type "Window : 895 x 1215mm" | names: "Window : 895 x 1215mm : 22" | material: "Window Default"
          1 x IFCSLAB | type IFCSLABTYPE "Floor : 100mm" | object type "Floor : 100mm" | FLOOR | names: "Floor : 100mm" | material: layers "Floor : 100mm" ("Floor default" 0.1) | property sets: Pset_SlabCommon, Pset_ReinforcementBarPitchOfSlab, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Covering : 20mm" | object type "Covering : 20mm" | CEILING | names: "Covering : 20mm" | material: layers "Covering : 20mm" ("Covering default" 0.02)
        IFCSPACE "Room 006"
        IFCSPACE "Room 007"
        IFCSPACE "Room 008"
        IFCSPACE "Room 009"

Types
  IFCWALLTYPE "wall_thickness_0.2000" | STANDARD | 44 occurrences | material: layers "wall_thickness_0.2000" ("Default wall" 0.200000002980232) | property sets: Pset_WallCommon
  IFCWINDOWSTYLE "Window : 880 x 1210mm" | 4 occurrences | material: "Window Default" | property sets: Window : 880 x 1210mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 920 x 1225mm" | 2 occurrences | material: "Window Default" | property sets: Window : 920 x 1225mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 1010 x 2100mm" | SINGLE_SWING_RIGHT | 3 occurrences | material: "Door Panel" | property sets: Door : 1010 x 2100mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 920 x 1220mm" | 1 occurrence | material: "Window Default" | property sets: Window : 920 x 1220mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 1010 x 2105mm" | SINGLE_SWING_RIGHT | 3 occurrences | material: "Door Panel" | property sets: Door : 1010 x 2105mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 945 x 1225mm" | 1 occurrence | material: "Window Default" | property sets: Window : 945 x 1225mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 900 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 900 x 1215mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 905 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 905 x 1215mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 925 x 1225mm" | 2 occurrences | material: "Window Default" | property sets: Window : 925 x 1225mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 720 x 2125mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Door Panel" | property sets: Door : 720 x 2125mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 915 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 915 x 1215mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 915 x 1220mm" | 1 occurrence | material: "Window Default" | property sets: Window : 915 x 1220mm, Pset_WindowCommon
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCWINDOWSTYLE "Window : 925 x 1235mm" | 4 occurrences | material: "Window Default" | property sets: Window : 925 x 1235mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 910 x 1225mm" | 3 occurrences | material: "Window Default" | property sets: Window : 910 x 1225mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 880 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 880 x 1215mm, Pset_WindowCommon
  IFCDOORSTYLE "Door : 1005 x 2100mm" | SINGLE_SWING_RIGHT | 2 occurrences | material: "Door Panel" | property sets: Door : 1005 x 2100mm, Pset_DoorCommon
  IFCWINDOWSTYLE "Window : 925 x 1230mm" | 1 occurrence | material: "Window Default" | property sets: Window : 925 x 1230mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 890 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 890 x 1215mm, Pset_WindowCommon
  IFCWINDOWSTYLE "Window : 895 x 1215mm" | 1 occurrence | material: "Window Default" | property sets: Window : 895 x 1215mm, Pset_WindowCommon
  IFCSLABTYPE "Floor : 100mm" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Covering : 20mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon

Property sets
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 1.E+20 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor : 100mm" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor : 100mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 43.2874 [SQUARE_METRE]
    GrossPerimeter = 28.8879 [METRE]
    GrossVolume = 171.0151 [CUBIC_METRE]
    Height = 3.9507 [METRE]
    NetFloorArea = 43.2874 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 49.9012 [SQUARE_METRE]
    GrossPerimeter = 28.8052 [METRE]
    GrossVolume = 197.144 [CUBIC_METRE]
    Height = 3.9507 [METRE]
    NetFloorArea = 49.9012 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 121.1938 [SQUARE_METRE]
    GrossPerimeter = 54.5169 [METRE]
    GrossVolume = 478.7989 [CUBIC_METRE]
    Height = 3.9507 [METRE]
    NetFloorArea = 121.1938 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 53.0193 [SQUARE_METRE]
    GrossPerimeter = 29.2224 [METRE]
    GrossVolume = 209.4626 [CUBIC_METRE]
    Height = 3.9507 [METRE]
    NetFloorArea = 53.0193 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 12.7923 [SQUARE_METRE]
    GrossPerimeter = 16.7973 [METRE]
    GrossVolume = 50.5384 [CUBIC_METRE]
    Height = 3.9507 [METRE]
    NetFloorArea = 12.7923 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 189.9768 [SQUARE_METRE]
    GrossPerimeter = 59.2015 [METRE]
    GrossVolume = 722.0548 [CUBIC_METRE]
    Height = 3.8008 [METRE]
    NetFloorArea = 189.9768 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 53.0143 [SQUARE_METRE]
    GrossPerimeter = 29.2212 [METRE]
    GrossVolume = 201.4941 [CUBIC_METRE]
    Height = 3.8008 [METRE]
    NetFloorArea = 53.0143 [SQUARE_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 26.8287 [SQUARE_METRE]
    GrossPerimeter = 29.0078 [METRE]
    GrossVolume = 101.9692 [CUBIC_METRE]
    Height = 3.8008 [METRE]
    NetFloorArea = 26.8287 [SQUARE_METRE]
  BaseQuantities: 1 more content on 1 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "wall_thickness_0.2000" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "wall_thickness_0.2000" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Window : 880 x 1210mm | predefined | on 1 type object
  Pset_WindowCommon | properties | on 15 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 920 x 1225mm | predefined | on 1 type object
  Door : 1010 x 2100mm | predefined | on 2 type objects
  Pset_DoorCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Window : 920 x 1220mm | predefined | on 1 type object
  Door : 1010 x 2105mm | predefined | on 2 type objects
  Window : 945 x 1225mm | predefined | on 1 type object
  Window : 900 x 1215mm | predefined | on 1 type object
  Window : 905 x 1215mm | predefined | on 1 type object
  Window : 925 x 1225mm | predefined | on 1 type object
  Door : 720 x 2125mm | predefined | on 2 type objects
  Window : 915 x 1215mm | predefined | on 1 type object
  Window : 915 x 1220mm | predefined | on 1 type object
  Pset_CoveringCommon | properties | on 9 type objects
    TotalThickness = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Window : 925 x 1235mm | predefined | on 1 type object
  Window : 910 x 1225mm | predefined | on 1 type object
  Window : 880 x 1215mm | predefined | on 1 type object
  Door : 1005 x 2100mm | predefined | on 2 type objects
  Window : 925 x 1230mm | predefined | on 1 type object
  Window : 890 x 1215mm | predefined | on 1 type object
  Window : 895 x 1215mm | predefined | on 1 type object